**Different directions:**

{

command\_id: 16,

navigation: (int) (0-straight, 1-left, 2-right, 3- U-turn, 4-Slight left, 5-Slight right)

}

**Straight, continue straight, round about continue straight-** Both the straps vibrates

**Left, circle left-** Left strap will vibrate continuously without any delay

**Right, circle right-** Right strap will vibrate continuously without any delay

**U-turn-** vibrate both straps with some delay

**Slight left lane, keep left-** vibrate left strap alone with some delay

**Slight Right lane, keep right-** vibrate right strap with some delay