**Phone to bag:**

**Predefined animation:**

{"command\_id":0,"animation\_id":5,"display\_mode":0}

**Entering text:**

{"command\_id":2,"num\_chars":5,"intensity":10,"frame\_delay":100,"text":"hello","led\_ring\_str":["0x00ffff"]}

**Printing the time (rtc):**

{"command\_id":10,"get\_time": ['5','37']}

**Beacon missing:**

{"command\_id":7,"addresses":["fc:58:fa:89:af:fa","35:57:fc:2e:70:8a"],"num\_beacons":2}

**Charge capacity:**

{"command\_id":9,"charge\_mode\_doc":0,"charge\_capacity\_doc":15000,"current\_capacity\_doc":200}

**Inner illumination:**

{"command\_id":4,"inner\_illumination":1}

**Custom animation:**

{"command\_id":1,"num\_frames":10,"display\_mode":0,"frame\_delay":[100,100,100,100,100,100,100,100,100,100],"led\_frames":["0x0148001918800210","0x1000821818018009","0x20040018990000a4","0x9000029818010048","0x0148001918800210","0x1000821818018009","0x20040018990000a4","0x20040018990000a4","0x0148001918800210","0x0148001918800210"],"intensities":[15,15,15,15,15,15,15,15,15,15],"led\_ring\_str":["0xffffff"]}

**Secure mode:**

{"command\_id":5,"secure\_mode":0}

**Deep sleep:**

{"command\_id":6,"data":0}